NCP81172 Evaluation Board User Guide

Preparation for use:
[bookmark: _GoBack]1. Connect input supply to J74 (+) and J71 (-). Supply can range from 4.5 V to 24 V; +12 V recommended.
2. Connect +5 V to J73, negative to pin 1 and positive to pin 2. This powers the NCP81172’s drivers and the EVB logic.
3. Short JP19 and JP20, unless using current sensing resistors (R190 and R194).
4. Select operating mode by J78 header. Short pins 1 and 2 for PS0; open all pins for PS1; short pins 2 and 3 for PS2.
5. Short pins 1 and 2 of J85 header to put EVB in non-standby mode.
6. Make sure that R204 is 0 ohms, and R225 is not populated.

Powering Up and Operation
1. Once the input power and +5 V power are connected, turn on the supplies, in no particular order.
2. Turn on the switch to the left to turn on the EVB. The green LED should light up, and the output should be at 0.9 V.

Unfortunately, no physical boards can be found, so no pictures are available.
