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DevSuite Software - External Release Notes for 6.1.32
(Version 6.1.32.59496 - build date 08/07/2023)
Special Notices
· Starting with Release 6.0.37
· Due to a change in one of our support libraries, ALL software must be uninstalled and installers rerun.

· This only has to be performed one time.

· Installers can be at different revisions, but at a minimum must be at 6.0.37.
Known Issues

· None.
Changes for Release 6.1.32
· New Sensor Support
· None. 
· New Features

· Added a STATE variable to allow still filename auto-increment to increment by any amount, instead of always 1.

· General Changes
· Added data_size attribute to Python Register class.
· Added OTPM lookup features (otpm_registers_by_name and Tools
· otpm_registers_by_address) to the Sensor and Register Python classes. 
· Fix 16-channel software lens shading calibration causing too much gain in the Account for mission or empty CSV file.correction (two issues). Some clean up in colorpipe level. 
· Fix crash if data is companded, and still averaging is selected, and decompand still images is not selected.
· In Poll Frame Buffer mode, use the timeout programmed in midlib instead of hardcoded 5000ms.
· Documentation

· Added the EXE that points to the Confluence SERDES User Guide documentation. 
· FlasTtool
· None for this release.

· Register Wizard
· None for this release.
· SensorTune

· None for this release.
Installation Instructions

Refer to the “DevSuite Quick-Start Guide” for installation and usage instructions. It can be found via the Startup shortcut “All Programs / Aptina Imaging”.
To Create Bug Reports and Feature Requests: 

Click the bug report button [image: image1.png]


 on DevWareX.
Use this link for instructions on how to gather “Crash” information.
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